## This file is a general .xdc for the Nexys4 rev B board
## To use it in a project:
## - uncomment the lines corresponding to used pins
## - rename the used ports (in each line, after get_ports) according to the top level signal names in the project

## Clock signal
##Bank = 35, Pin name = IO_L12P_T1_MRCC_35,					Sch Wname = CLK100MHZ
set_property PACKAGE_PIN E3 [get_ports clk]
	set_property IOSTANDARD LVCMOS33 [get_ports clk]
	create_clock -add -name clk -period 10.00 -waveform {0 5} [get_ports clk]

## Switches
##Bank = 34, Pin name = IO_L21P_T3_DQS_34,					Sch name = SW0
 set_property PACKAGE_PIN U9 [get_ports {sw[0]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {sw[0]}]
##Bank = 34, Pin name = IO_25_34,							Sch name = SW1
set_property PACKAGE_PIN U8 [get_ports {sw[1]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {sw[1]}]
##Bank = 34, Pin name = IO_L23P_T3_34,						Sch name = SW2
set_property PACKAGE_PIN R7 [get_ports {sw[2]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {sw[2]}]
##Bank = 34, Pin name = IO_L19P_T3_34,						Sch name = SW3
set_property PACKAGE_PIN R6 [get_ports {sw[3]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {sw[3]}]
##Bank = 34, Pin name = IO_L19N_T3_VREF_34,					Sch name = SW4
set_property PACKAGE_PIN R5 [get_ports {sw[4]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {sw[4]}]
##Bank = 34, Pin name = IO_L20P_T3_34,						Sch name = SW5
set_property PACKAGE_PIN V7 [get_ports {sw[5]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {sw[5]}]
##Bank = 34, Pin name = IO_L20N_T3_34,						Sch name = SW6
set_property PACKAGE_PIN V6 [get_ports {sw[6]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {sw[6]}]
##Bank = 34, Pin name = IO_L10P_T1_34,						Sch name = SW7
set_property PACKAGE_PIN V5 [get_ports {sw[7]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {sw[7]}]
##Bank = 34, Pin name = IO_L8P_T1-34,						Sch name = SW8
#set_property PACKAGE_PIN U4 [get_ports {sw[8]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {sw[8]}]
##Bank = 34, Pin name = IO_L9N_T1_DQS_34,					Sch name = SW9
#set_property PACKAGE_PIN V2 [get_ports {sw[9]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {sw[9]}]
##Bank = 34, Pin name = IO_L9P_T1_DQS_34,					Sch name = SW10
#set_property PACKAGE_PIN U2 [get_ports {sw[10]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {sw[10]}]
##Bank = 34, Pin name = IO_L11N_T1_MRCC_34,					Sch name = SW11
#set_property PACKAGE_PIN T3 [get_ports {sw[11]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {sw[11]}]
##Bank = 34, Pin name = IO_L17N_T2_34,						Sch name = SW12
#set_property PACKAGE_PIN T1 [get_ports {sw[12]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {sw[12]}]
##Bank = 34, Pin name = IO_L11P_T1_SRCC_34,					Sch name = SW13
#set_property PACKAGE_PIN R3 [get_ports {sw[13]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {sw[13]}]
##Bank = 34, Pin name = IO_L14N_T2_SRCC_34,					Sch name = SW14
#set_property PACKAGE_PIN P3 [get_ports {sw[14]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {sw[14]}]
##Bank = 34, Pin name = IO_L14P_T2_SRCC_34,					Sch name = SW15
#set_property PACKAGE_PIN P4 [get_ports {sw[15]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {sw[15]}]



## LEDs
##Bank = 34, Pin name = IO_L24N_T3_34,						Sch name = LED0
set_property PACKAGE_PIN T8 [get_ports {led[0]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {led[0]}]
#Bank = 34, Pin name = IO_L21N_T3_DQS_34,					Sch name = LED1
set_property PACKAGE_PIN V9 [get_ports {led[1]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {led[1]}]
#Bank = 34, Pin name = IO_L24P_T3_34,						Sch name = LED2
 set_property PACKAGE_PIN R8 [get_ports {led[2]}]
 	set_property IOSTANDARD LVCMOS33 [get_ports {led[2]}]
#Bank = 34, Pin name = IO_L23N_T3_34,						Sch name = LED3
 set_property PACKAGE_PIN T6 [get_ports {led[3]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {led[3]}]
#Bank = 34, Pin name = IO_L12P_T1_MRCC_34,					Sch name = LED4
set_property PACKAGE_PIN T5 [get_ports {led[4]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {led[4]}]
#Bank = 34, Pin name = IO_L12N_T1_MRCC_34,					Sch	name = LED5
set_property PACKAGE_PIN T4 [get_ports {led[5]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {led[5]}]
#Bank = 34, Pin name = IO_L22P_T3_34,						Sch name = LED6
set_property PACKAGE_PIN U7 [get_ports {led[6]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {led[6]}]
#Bank = 34, Pin name = IO_L22N_T3_34,						Sch name = LED7
set_property PACKAGE_PIN U6 [get_ports {led[7]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {led[7]}]
#Bank = 34, Pin name = IO_L10N_T1_34,						Sch name = LED8
set_property PACKAGE_PIN V4 [get_ports {debug[0]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {debug[0]}]
#Bank = 34, Pin name = IO_L8N_T1_34,						Sch name = LED9
set_property PACKAGE_PIN U3 [get_ports {debug[1]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {debug[1]}]
#Bank = 34, Pin name = IO_L7N_T1_34,						Sch name = LED10
set_property PACKAGE_PIN V1 [get_ports {debug[2]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {debug[2]}]
#Bank = 34, Pin name = IO_L17P_T2_34,						Sch name = LED11
set_property PACKAGE_PIN R1 [get_ports {debug[3]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {debug[3]}]
#Bank = 34, Pin name = IO_L13N_T2_MRCC_34,					Sch name = LED12
set_property PACKAGE_PIN P5 [get_ports {debug[4]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {debug[4]}]
#Bank = 34, Pin name = IO_L7P_T1_34,						Sch name = LED13
set_property PACKAGE_PIN U1 [get_ports {debug[5]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {debug[5]}]
#Bank = 34, Pin name = IO_L15N_T2_DQS_34,					Sch name = LED14
set_property PACKAGE_PIN R2 [get_ports {debug[6]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {debug[6]}]
#Bank = 34, Pin name = IO_L15P_T2_DQS_34,					Sch name = LED15
set_property PACKAGE_PIN P2 [get_ports {debug[7]}]
	set_property IOSTANDARD LVCMOS33 [get_ports {debug[7]}]

##Bank = 34, Pin name = IO_L5P_T0_34,						Sch name = LED16_R
#set_property PACKAGE_PIN K5 [get_ports {rgb[0]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {rgb[0]}]
##Bank = 15, Pin name = IO_L5P_T0_AD9P_15,					Sch name = LED16_G
#set_property PACKAGE_PIN F13 [get_ports {rgb[1]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {rgb[1]}]
##Bank = 35, Pin name = IO_L19N_T3_VREF_35,					Sch name = LED16_B
#set_property PACKAGE_PIN F6 [get_ports {rgb[2]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {rgb[2]}]
##Bank = 34, Pin name = IO_0_34,								Sch name = LED17_R
#set_property PACKAGE_PIN K6 [get_ports {rgb[3]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {rgb[3]}]
##Bank = 35, Pin name = IO_24P_T3_35,						Sch name =  LED17_G
#set_property PACKAGE_PIN H6 [get_ports {rgb[4]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {rgb[4]}]
##Bank = CONFIG, Pin name = IO_L3N_T0_DQS_EMCCLK_14,			Sch name = LED17_B
#set_property PACKAGE_PIN L16 [get_ports {rgb[5]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {rgb[5]}]



##7 segment display
##Bank = 34, Pin name = IO_L2N_T0_34,						Sch name = CA
#set_property PACKAGE_PIN L3 [get_ports {seg[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {seg[0]}]
##Bank = 34, Pin name = IO_L3N_T0_DQS_34,					Sch name = CB
#set_property PACKAGE_PIN N1 [get_ports {seg[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {seg[1]}]
##Bank = 34, Pin name = IO_L6N_T0_VREF_34,					Sch name = CC
#set_property PACKAGE_PIN L5 [get_ports {seg[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {seg[2]}]
##Bank = 34, Pin name = IO_L5N_T0_34,						Sch name = CD
#set_property PACKAGE_PIN L4 [get_ports {seg[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {seg[3]}]
##Bank = 34, Pin name = IO_L2P_T0_34,						Sch name = CE
#set_property PACKAGE_PIN K3 [get_ports {seg[4]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {seg[4]}]
##Bank = 34, Pin name = IO_L4N_T0_34,						Sch name = CF
#set_property PACKAGE_PIN M2 [get_ports {seg[5]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {seg[5]}]
##Bank = 34, Pin name = IO_L6P_T0_34,						Sch name = CG
#set_property PACKAGE_PIN L6 [get_ports {seg[6]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {seg[6]}]

##Bank = 34, Pin name = IO_L16P_T2_34,						Sch name = DP
#set_property PACKAGE_PIN M4 [get_ports dp]
	#set_property IOSTANDARD LVCMOS33 [get_ports dp]

##Bank = 34, Pin name = IO_L18N_T2_34,						Sch name = AN0
#set_property PACKAGE_PIN N6 [get_ports {an[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {an[0]}]
##Bank = 34, Pin name = IO_L18P_T2_34,						Sch name = AN1
#set_property PACKAGE_PIN M6 [get_ports {an[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {an[1]}]
##Bank = 34, Pin name = IO_L4P_T0_34,						Sch name = AN2
#set_property PACKAGE_PIN M3 [get_ports {an[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {an[2]}]
##Bank = 34, Pin name = IO_L13_T2_MRCC_34,					Sch name = AN3
#set_property PACKAGE_PIN N5 [get_ports {an[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {an[3]}]
##Bank = 34, Pin name = IO_L3P_T0_DQS_34,					Sch name = AN4
#set_property PACKAGE_PIN N2 [get_ports {an[4]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {an[4]}]
##Bank = 34, Pin name = IO_L16N_T2_34,						Sch name = AN5
#set_property PACKAGE_PIN N4 [get_ports {an[5]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {an[5]}]
##Bank = 34, Pin name = IO_L1P_T0_34,						Sch name = ANyte_out6
#set_property PACKAGE_PIN L1 [get_ports {an[6]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {an[6]}]
##Bank = 34, Pin name = IO_L1N_T034,							Sch name = AN7
#set_property PACKAGE_PIN M1 [get_ports {an[7]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {an[7]}]



##Buttons
##Bank = 15, Pin name = IO_L3P_T0_DQS_AD1P_15,				Sch name = CPU_RESET
#set_property PACKAGE_PIN C12 [get_ports reset]
#	set_property IOSTANDARD LVCMOS33 [get_ports reset]
##Bank = 15, Pin name = IO_L11N_T1_SRCC_15,					Sch name = BTNC
#set_property PACKAGE_PIN E16 [get_ports clk]
#	set_property IOSTANDARD LVCMOS33 [get_ports clk]
##Bank = 15, Pin name = IO_L14P_T2_SRCC_15,					Sch name = BTNU
#set_property PACKAGE_PIN F15 [get_ports btnU]
	#set_property IOSTANDARD LVCMOS33 [get_ports btnU]
##Bank = CONFIG, Pin name = IO_L15N_T2_DQS_DOUT_CSO_B_14,	Sch name = BTNL
#set_property PACKAGE_PIN T16 [get_ports btnL]
	#set_property IOSTANDARD LVCMOS33 [get_ports btnL]
##Bank = 14, Pin name = IO_25_14,							Sch name = BTNR
#set_property PACKAGE_PIN R10 [get_ports btnR]
	#set_property IOSTANDARD LVCMOS33 [get_ports btnR]
##Bank = 14, Pin name = IO_L21P_T3_DQS_14,					Sch name = BTND
#set_property PACKAGE_PIN V10 [get_ports btnD]
	#set_property IOSTANDARD LVCMOS33 [get_ports btnD]



##Pmod Header JA
##Bank = 15, Pin name = IO_L1N_T0_AD0N_15,					Sch name = JA1
#set_property PACKAGE_PIN B13 [get_ports {JA[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JA[0]}]
##Bank = 15, Pin name = IO_L5N_T0_AD9N_15,					Sch name = JA2
#set_property PACKAGE_PIN F14 [get_ports {JA[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JA[1]}]
##Bank = 15, Pin name = IO_L16N_T2_A27_15,					Sch name = JA3
#set_property PACKAGE_PIN D17 [get_ports {JA[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JA[2]}]
##Bank = 15, Pin name = IO_L16P_T2_A28_15,					Sch name = JA4
#set_property PACKAGE_PIN E17 [get_ports {JA[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JA[3]}]
##Bank = 15, Pin name = IO_0_15,								Sch name = JA7
#set_property PACKAGE_PIN G13 [get_ports {JA[4]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JA[4]}]
##Bank = 15, Pin name = IO_L20N_T3_A19_15,					Sch name = JA8
#set_property PACKAGE_PIN C17 [get_ports {JA[5]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JA[5]}]
##Bank = 15, Pin name = IO_L21N_T3_A17_15,					Sch name = JA9
#set_property PACKAGE_PIN D18 [get_ports {JA[6]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JA[6]}]
##Bank = 15, Pin name = IO_L21P_T3_DQS_15,					Sch name = JA10
#set_property PACKAGE_PIN E18 [get_ports {JA[7]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JA[7]}]



##Pmod Header JB
##Bank = 15, Pin name = IO_L15N_T2_DQS_ADV_B_15,				Sch name = JB1
#set_property PACKAGE_PIN G14 [get_ports {JB[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JB[0]}]
##Bank = 14, Pin name = IO_L13P_T2_MRCC_14,					Sch name = JB2
#set_property PACKAGE_PIN P15 [get_ports {JB[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JB[1]}]
##Bank = 14, Pin name = IO_L21N_T3_DQS_A06_D22_14,			Sch name = JB3
#set_property PACKAGE_PIN V11 [get_ports {JB[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JB[2]}]
##Bank = CONFIG, Pin name = IO_L16P_T2_CSI_B_14,				Sch name = JB4
#set_property PACKAGE_PIN V15 [get_ports {JB[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JB[3]}]
##Bank = 15, Pin name = IO_25_15,							Sch name = JB7
#set_property PACKAGE_PIN K16 [get_ports {JB[4]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JB[4]}]
##Bank = CONFIG, Pin name = IO_L15P_T2_DQS_RWR_B_14,			Sch name = JB8
#set_property PACKAGE_PIN R16 [get_ports {JB[5]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JB[5]}]
##Bank = 14, Pin name = IO_L24P_T3_A01_D17_14,				Sch name = JB9
#set_property PACKAGE_PIN T9 [get_ports {JB[6]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JB[6]}]
##Bank = 14, Pin name = IO_L19N_T3_A09_D25_VREF_14,			Sch name = JB10
#set_property PACKAGE_PIN U11 [get_ports {JB[7]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JB[7]}]



##Pmod Header JC
##Bank = 35, Pin name = IO_L23P_T3_35,						Sch name = JC1
#set_property PACKAGE_PIN K2 [get_ports {JC[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JC[0]}]
##Bank = 35, Pin name = IO_L6P_T0_35,						Sch name = JC2
#set_property PACKAGE_PIN E7 [get_ports {JC[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JC[1]}]
##Bank = 35, Pin name = IO_L22P_T3_35,						Sch name = JC3
#set_property PACKAGE_PIN J3 [get_ports {JC[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JC[2]}]
##Bank = 35, Pin name = IO_L21P_T3_DQS_35,					Sch name = JC4
#set_property PACKAGE_PIN J4 [get_ports {JC[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JC[3]}]
##Bank = 35, Pin name = IO_L23N_T3_35,						Sch name = JC7
#set_property PACKAGE_PIN K1 [get_ports {JC[4]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JC[4]}]
##Bank = 35, Pin name = IO_L5P_T0_AD13P_35,					Sch name = JC8
#set_property PACKAGE_PIN E6 [get_ports {JC[5]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JC[5]}]
##Bank = 35, Pin name = IO_L22N_T3_35,						Sch name = JC9
#set_property PACKAGE_PIN J2 [get_ports {JC[6]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JC[6]}]
##Bank = 35, Pin name = IO_L19P_T3_35,						Sch name = JC10
#set_property PACKAGE_PIN G6 [get_ports {JC[7]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JC[7]}]



##Pmod Header JD
##Bank = 35, Pin name = IO_L21N_T2_DQS_35,					Sch name = JD1
#set_property PACKAGE_PIN H4 [get_ports {JD[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JD[0]}]
##Bank = 35, Pin name = IO_L17P_T2_35,						Sch name = JD2
#set_property PACKAGE_PIN H1 [get_ports {JD[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JD[1]}]
##Bank = 35, Pin name = IO_L17N_T2_35,						Sch name = JD3
#set_property PACKAGE_PIN G1 [get_ports {JD[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JD[2]}]
##Bank = 35, Pin name = IO_L20N_T3_35,						Sch name = JD4
#set_property PACKAGE_PIN G3 [get_ports {JD[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JD[3]}]
##Bank = 35, Pin name = IO_L15P_T2_DQS_35,					Sch name = JD7
#set_property PACKAGE_PIN H2 [get_ports {JD[4]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JD[4]}]
##Bank = 35, Pin name = IO_L20P_T3_35,						Sch name = JD8
#set_property PACKAGE_PIN G4 [get_ports {JD[5]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JD[5]}]
##Bank = 35, Pin name = IO_L15N_T2_DQS_35,					Sch name = JD9
#set_property PACKAGE_PIN G2 [get_ports {JD[6]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JD[6]}]
##Bank = 35, Pin name = IO_L13N_T2_MRCC_35,					Sch name = JD10
#set_property PACKAGE_PIN F3 [get_ports {JD[7]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JD[7]}]



##Pmod Header JXADC
##Bank = 15, Pin name = IO_L9P_T1_DQS_AD3P_15,				Sch name = XADC1_P -> XA1_P
#set_property PACKAGE_PIN A13 [get_ports {JXADC[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JXADC[0]}]
##Bank = 15, Pin name = IO_L8P_T1_AD10P_15,					Sch name = XADC2_P -> XA2_P
#set_property PACKAGE_PIN A15 [get_ports {JXADC[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JXADC[1]}]
##Bank = 15, Pin name = IO_L7P_T1_AD2P_15,					Sch name = XADC3_P -> XA3_P
#set_property PACKAGE_PIN B16 [get_ports {JXADC[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JXADC[2]}]
##Bank = 15, Pin name = IO_L10P_T1_AD11P_15,					Sch name = XADC4_P -> XA4_P
#set_property PACKAGE_PIN B18 [get_ports {JXADC[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JXADC[3]}]
##Bank = 15, Pin name = IO_L9N_T1_DQS_AD3N_15,				Sch name = XADC1_N -> XA1_N
#set_property PACKAGE_PIN A14 [get_ports {JXADC[4]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JXADC[4]}]
##Bank = 15, Pin name = IO_L8N_T1_AD10N_15,					Sch name = XADC2_N -> XA2_N
#set_property PACKAGE_PIN A16 [get_ports {JXADC[5]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JXADC[5]}]
##Bank = 15, Pin name = IO_L7N_T1_AD2N_15,					Sch name = XADC3_N -> XA3_N
#set_property PACKAGE_PIN B17 [get_ports {JXADC[6]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JXADC[6]}]
##Bank = 15, Pin name = IO_L10N_T1_AD11N_15,					Sch name = XADC4_N -> XA4_N
#set_property PACKAGE_PIN A18 [get_ports {JXADC[7]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {JXADC[7]}]



##VGA Connector
##Bank = 35, Pin name = IO_L8N_T1_AD14N_35,					Sch name = VGA_R0
#set_property PACKAGE_PIN A3 [get_ports {vgaRed[0]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {vgaRed[0]}]
##Bank = 35, Pin name = IO_L7N_T1_AD6N_35,					Sch name = VGA_R1
#set_property PACKAGE_PIN B4 [get_ports {vgaRed[1]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {vgaRed[1]}]
##Bank = 35, Pin name = IO_L1N_T0_AD4N_35,					Sch name = VGA_R2
#set_property PACKAGE_PIN C5 [get_ports {vgaRed[2]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {vgaRed[2]}]
##Bank = 35, Pin name = IO_L8P_T1_AD14P_35,					Sch name = VGA_R3
#set_property PACKAGE_PIN A4 [get_ports {vgaRed[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {vgaRed[3]}]
##Bank = 35, Pin name = IO_L2P_T0_AD12P_35,					Sch name = VGA_B0
#set_property PACKAGE_PIN B7 [get_ports {vgaBlue[0]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {vgaBlue[0]}]
##Bank = 35, Pin name = IO_L4N_T0_35,						Sch name = VGA_B1
#set_property PACKAGE_PIN C7 [get_ports {vgaBlue[1]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {vgaBlue[1]}]
##Bank = 35, Pin name = IO_L6N_T0_VREF_35,					Sch name = VGA_B2
#set_property PACKAGE_PIN D7 [get_ports {vgaBlue[2]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {vgaBlue[2]}]
##Bank = 35, Pin name = IO_L4P_T0_35,						Sch name = VGA_B3
#set_property PACKAGE_PIN D8 [get_ports {vgaBlue[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {vgaBlue[3]}]
##Bank = 35, Pin name = IO_L1P_T0_AD4P_35,					Sch name = VGA_G0
#set_property PACKAGE_PIN C6 [get_ports {vgaGreen[0]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {vgaGreen[0]}]
##Bank = 35, Pin name = IO_L3N_T0_DQS_AD5N_35,				Sch name = VGA_G1
#set_property PACKAGE_PIN A5 [get_ports {vgaGreen[1]}]
#	set_property IOSTANDARD LVCMOS33 [get_ports {vgaGreen[1]}]
##Bank = 35, Pin name = IO_L2N_T0_AD12N_35,					Sch name = VGA_G2
#set_property PACKAGE_PIN B6 [get_ports {vgaGreen[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {vgaGreen[2]}]
##Bank = 35, Pin name = IO_L3P_T0_DQS_AD5P_35,				Sch name = VGA_G3
#set_property PACKAGE_PIN A6 [get_ports {vgaGreen[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {vgaGreen[3]}]
##Bank = 15, Pin name = IO_L4P_T0_15,						Sch name = VGA_HS
#set_property PACKAGE_PIN B11 [get_ports Hsync]
#	set_property IOSTANDARD LVCMOS33 [get_ports Hsync]
##Bank = 15, Pin name = IO_L3N_T0_DQS_AD1N_15,				Sch name = VGA_VS
#set_property PACKAGE_PIN B12 [get_ports Vsync]
#	set_property IOSTANDARD LVCMOS33 [get_ports Vsync]



##Micro SD Connector
##Bank = 35, Pin name = IO_L14P_T2_SRCC_35,					Sch name = SD_RESET
#set_property PACKAGE_PIN E2 [get_ports sdReset]
	#set_property IOSTANDARD LVCMOS33 [get_ports sdReset]
##Bank = 35, Pin name = IO_L9N_T1_DQS_AD7N_35,				Sch name = SD_CD
#set_property PACKAGE_PIN A1 [get_ports sdCD]
	#set_property IOSTANDARD LVCMOS33 [get_ports sdCD]
##Bank = 35, Pin name = IO_L9P_T1_DQS_AD7P_35,				Sch name = SD_SCK
#set_property PACKAGE_PIN B1 [get_ports sdSCK]
	#set_property IOSTANDARD LVCMOS33 [get_ports sdSCK]
##Bank = 35, Pin name = IO_L16N_T2_35,						Sch name = SD_CMD
#set_property PACKAGE_PIN C1 [get_ports sdCmd]
	#set_property IOSTANDARD LVCMOS33 [get_ports sdCmd]
##Bank = 35, Pin name = IO_L16P_T2_35,						Sch name = SD_DAT0
#set_property PACKAGE_PIN C2 [get_ports {sdData[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {sdData[0]}]
##Bank = 35, Pin name = IO_L18N_T2_35,						Sch name = SD_DAT1
#set_property PACKAGE_PIN E1 [get_ports {sdData[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {sdData[1]}]
##Bank = 35, Pin name = IO_L18P_T2_35,						Sch name = SD_DAT2
#set_property PACKAGE_PIN F1 [get_ports {sdData[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {sdData[2]}]
##Bank = 35, Pin name = IO_L14N_T2_SRCC_35,					Sch name = SD_DAT3
#set_property PACKAGE_PIN D2 [get_ports {sdData[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {sdData[3]}]



##Accelerometer
##Bank = 15, Pin name = IO_L6N_T0_VREF_15,					Sch name = ACL_MISO
#set_property PACKAGE_PIN D13 [get_ports MISO]
#	set_property IOSTANDARD LVCMOS33 [get_ports MISO]
#Bank = 15, Pin name = IO_L2N_T0_AD8N_15,					Sch name = ACL_MOSI
#set_property PACKAGE_PIN B14 [get_ports MOSI]
#	set_property IOSTANDARD LVCMOS33 [get_ports MOSI]
#Bank = 15, Pin name = IO_L12P_T1_MRCC_15,					Sch name = ACL_SCLK
#set_property PACKAGE_PIN D15 [get_ports SCLK]
#	set_property IOSTANDARD LVCMOS33 [get_ports SCLK]
#Bank = 15, Pin name = IO_L12N_T1_MRCC_15,					Sch name = ACL_CSN
#set_property PACKAGE_PIN C15 [get_ports SS]
#	set_property IOSTANDARD LVCMOS33 [get_ports SS]
##Bank = 15, Pin name = IO_L20P_T3_A20_15,					Sch name = ACL_INT1
#set_property PACKAGE_PIN C16 [get_ports aclInt1]
	#set_property IOSTANDARD LVCMOS33 [get_ports aclInt1]
##Bank = 15, Pin name = IO_L11P_T1_SRCC_15,					Sch name = ACL_INT2
#set_property PACKAGE_PIN E15 [get_ports aclInt2]
	#set_property IOSTANDARD LVCMOS33 [get_ports aclInt2]



##Temperature Sensor
##Bank = 15, Pin name = IO_L14N_T2_SRCC_15,					Sch name = TMP_SCL
#set_property PACKAGE_PIN F16 [get_ports tmpSCL]
	#set_property IOSTANDARD LVCMOS33 [get_ports tmpSCL]
##Bank = 15, Pin name = IO_L13N_T2_MRCC_15,					Sch name = TMP_SDA
#set_property PACKAGE_PIN G16 [get_ports tmpSDA]
	#set_property IOSTANDARD LVCMOS33 [get_ports tmpSDA]
##Bank = 15, Pin name = IO_L1P_T0_AD0P_15,					Sch name = TMP_INT
#set_property PACKAGE_PIN D14 [get_ports tmpInt]
	#set_property IOSTANDARD LVCMOS33 [get_ports tmpInt]
##Bank = 15, Pin name = IO_L1N_T0_AD0N_15,					Sch name = TMP_CT
#set_property PACKAGE_PIN C14 [get_ports tmpCT]
	#set_property IOSTANDARD LVCMOS33 [get_ports tmpCT]



##Omnidirectional Microphone
##Bank = 35, Pin name = IO_25_35,							Sch name = M_CLK
#set_property PACKAGE_PIN J5 [get_ports micClk]
	#set_property IOSTANDARD LVCMOS33 [get_ports micClk]
##Bank = 35, Pin name = IO_L24N_T3_35,						Sch name = M_DATA
#set_property PACKAGE_PIN H5 [get_ports micData]
	#set_property IOSTANDARD LVCMOS33 [get_ports micData]
##Bank = 35, Pin name = IO_0_35,								Sch name = M_LRSEL
#set_property PACKAGE_PIN F5 [get_ports micLRSel]
	#set_property IOSTANDARD LVCMOS33 [get_ports micLRSel]



##PWM Audio Amplifier
##Bank = 15, Pin name = IO_L4N_T0_15,						Sch name = AUD_PWM
#set_property PACKAGE_PIN A11 [get_ports ampPWM]
	#set_property IOSTANDARD LVCMOS33 [get_ports ampPWM]
##Bank = 15, Pin name = IO_L6P_T0_15,						Sch name = AUD_SD
#set_property PACKAGE_PIN D12 [get_ports ampSD]
	#set_property IOSTANDARD LVCMOS33 [get_ports ampSD]


##USB-RS232 Interface
##Bank = 35, Pin name = IO_L7P_T1_AD6P_35,					Sch name = UART_TXD_IN
#set_property PACKAGE_PIN C4 [get_ports RsRx]
	#set_property IOSTANDARD LVCMOS33 [get_ports RsRx]
##Bank = 35, Pin name = IO_L11N_T1_SRCC_35,					Sch name = UART_RXD_OUT
#set_property PACKAGE_PIN D4 [get_ports RsTx]
	#set_property IOSTANDARD LVCMOS33 [get_ports RsTx]
##Bank = 35, Pin name = IO_L12N_T1_MRCC_35,					Sch name = UART_CTS
#set_property PACKAGE_PIN D3 [get_ports RsCts]
	#set_property IOSTANDARD LVCMOS33 [get_ports RsCts]
##Bank = 35, Pin name = IO_L5N_T0_AD13N_35,					Sch name = UART_RTS
#set_property PACKAGE_PIN E5 [get_ports RsRts]
	#set_property IOSTANDARD LVCMOS33 [get_ports RsRts]



##USB HID (PS/2)
##Bank = 35, Pin name = IO_L13P_T2_MRCC_35,					Sch name = PS2_CLK
#set_property PACKAGE_PIN F4 [get_ports PS2Clk]
	#set_property IOSTANDARD LVCMOS33 [get_ports PS2Clk]
	#set_property PULLUP true [get_ports PS2Clk]
##Bank = 35, Pin name = IO_L10N_T1_AD15N_35,					Sch name = PS2_DATA
#set_property PACKAGE_PIN B2 [get_ports PS2Data]
	#set_property IOSTANDARD LVCMOS33 [get_ports PS2Data]
	#set_property PULLUP true [get_ports PS2Data]



##SMSC Ethernet PHY
##Bank = 16, Pin name = IO_L11P_T1_SRCC_16,					Sch name = ETH_MDC
#set_property PACKAGE_PIN C9 [get_ports PhyMdc]
	#set_property IOSTANDARD LVCMOS33 [get_ports PhyMdc]
##Bank = 16, Pin name = IO_L14N_T2_SRCC_16,					Sch name = ETH_MDIO
#set_property PACKAGE_PIN A9 [get_ports PhyMdio]
	#set_property IOSTANDARD LVCMOS33 [get_ports PhyMdio]
##Bank = 35, Pin name = IO_L10P_T1_AD15P_35,					Sch name = ETH_RSTN
#set_property PACKAGE_PIN B3 [get_ports PhyRstn]
	#set_property IOSTANDARD LVCMOS33 [get_ports PhyRstn]
##Bank = 16, Pin name = IO_L6N_T0_VREF_16,					Sch name = ETH_CRSDV
#set_property PACKAGE_PIN D9 [get_ports PhyCrs]
	#set_property IOSTANDARD LVCMOS33 [get_ports PhyCrs]
##Bank = 16, Pin name = IO_L13N_T2_MRCC_16,					Sch name = ETH_RXERR
#set_property PACKAGE_PIN C10 [get_ports PhyRxErr]
	#set_property IOSTANDARD LVCMOS33 [get_ports PhyRxErr]
##Bank = 16, Pin name = IO_L19N_T3_VREF_16,					Sch name = ETH_RXD0
#set_property PACKAGE_PIN D10 [get_ports {PhyRxd[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {PhyRxd[0]}]
##Bank = 16, Pin name = IO_L13P_T2_MRCC_16,					Sch name = ETH_RXD1
#set_property PACKAGE_PIN C11 [get_ports {PhyRxd[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {PhyRxd[1]}]
##Bank = 16, Pin name = IO_L11N_T1_SRCC_16,					Sch name = ETH_TXEN
#set_property PACKAGE_PIN B9 [get_ports PhyTxEn]
	#set_property IOSTANDARD LVCMOS33 [get_ports PhyTxEn]
##Bank = 16, Pin name = IO_L14P_T2_SRCC_16,					Sch name = ETH_TXD0
#set_property PACKAGE_PIN A10 [get_ports {PhyTxd[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {PhyTxd[0]}]
##Bank = 16, Pin name = IO_L12N_T1_MRCC_16,					Sch name = ETH_TXD1
#set_property PACKAGE_PIN A8 [get_ports {PhyTxd[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {PhyTxd[1]}]
##Bank = 35, Pin name = IO_L11P_T1_SRCC_35,					Sch name = ETH_REFCLK
#set_property PACKAGE_PIN D5 [get_ports PhyClk50Mhz]
	#set_property IOSTANDARD LVCMOS33 [get_ports PhyClk50Mhz]
##Bank = 16, Pin name = IO_L12P_T1_MRCC_16,					Sch name = ETH_INTN
#set_property PACKAGE_PIN B8 [get_ports PhyIntn]
	#set_property IOSTANDARD LVCMOS33 [get_ports PhyIntn]



##Quad SPI Flash
##Bank = CONFIG, Pin name = CCLK_0,							Sch name = QSPI_SCK
#set_property PACKAGE_PIN E9 [get_ports {QspiSCK}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {QspiSCK}]
##Bank = CONFIG, Pin name = IO_L1P_T0_D00_MOSI_14,			Sch name = QSPI_DQ0
#set_property PACKAGE_PIN K17 [get_ports {QspiDB[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {QspiDB[0]}]
##Bank = CONFIG, Pin name = IO_L1N_T0_D01_DIN_14,			Sch name = QSPI_DQ1
#set_property PACKAGE_PIN K18 [get_ports {QspiDB[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {QspiDB[1]}]
##Bank = CONFIG, Pin name = IO_L20_T0_D02_14,				Sch name = QSPI_DQ2
#set_property PACKAGE_PIN L14 [get_ports {QspiDB[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {QspiDB[2]}]
##Bank = CONFIG, Pin name = IO_L2P_T0_D03_14,				Sch name = QSPI_DQ3
#set_property PACKAGE_PIN M14 [get_ports {QspiDB[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {QspiDB[3]}]
##Bank = CONFIG, Pin name = IO_L15N_T2_DQS_DOUT_CSO_B_14,	Sch name = QSPI_CSN
#set_property PACKAGE_PIN L13 [get_ports QspiCSn]
	#set_property IOSTANDARD LVCMOS33 [get_ports QspiCSn]



##Cellular RAM
##Bank = 14, Pin name = IO_L14N_T2_SRCC_14,					Sch name = CRAM_CLK
#set_property PACKAGE_PIN T15 [get_ports RamCLK]
	#set_property IOSTANDARD LVCMOS33 [get_ports RamCLK]
##Bank = 14, Pin name = IO_L23P_T3_A03_D19_14,				Sch name = CRAM_ADVN
#set_property PACKAGE_PIN T13 [get_ports RamADVn]
	#set_property IOSTANDARD LVCMOS33 [get_ports RamADVn]
##Bank = 14, Pin name = IO_L4P_T0_D04_14,					Sch name = CRAM_CEN
#set_property PACKAGE_PIN L18 [get_ports RamCEn]
	#set_property IOSTANDARD LVCMOS33 [get_ports RamCEn]
##Bank = 15, Pin name = IO_L19P_T3_A22_15,					Sch name = CRAM_CRE
#set_property PACKAGE_PIN J14 [get_ports RamCRE]
	#set_property IOSTANDARD LVCMOS33 [get_ports RamCRE]
##Bank = 15, Pin name = IO_L15P_T2_DQS_15,					Sch name = CRAM_OEN
#set_property PACKAGE_PIN H14 [get_ports RamOEn]
	#set_property IOSTANDARD LVCMOS33 [get_ports RamOEn]
##Bank = 14, Pin name = IO_0_14,								Sch name = CRAM_WEN
#set_property PACKAGE_PIN R11 [get_ports RamWEn]
	#set_property IOSTANDARD LVCMOS33 [get_ports RamWEn]
##Bank = 15, Pin name = IO_L24N_T3_RS0_15,					Sch name = CRAM_LBN
#set_property PACKAGE_PIN J15 [get_ports RamLBn]
	#set_property IOSTANDARD LVCMOS33 [get_ports RamLBn]
##Bank = 15, Pin name = IO_L17N_T2_A25_15,					Sch name = CRAM_UBN
#set_property PACKAGE_PIN J13 [get_ports RamUBn]
	#set_property IOSTANDARD LVCMOS33 [get_ports RamUBn]
##Bank = 14, Pin name = IO_L14P_T2_SRCC_14,					Sch name = CRAM_WAIT
#set_property PACKAGE_PIN T14 [get_ports RamWait]
	#set_property IOSTANDARD LVCMOS33 [get_ports RamWait]

##Bank = 14, Pin name = IO_L5P_T0_DQ06_14,					Sch name = CRAM_DQ0
#set_property PACKAGE_PIN R12 [get_ports {MemDB[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[0]}]
##Bank = 14, Pin name = IO_L19P_T3_A10_D26_14,				Sch name = CRAM_DQ1
#set_property PACKAGE_PIN T11 [get_ports {MemDB[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[1]}]
##Bank = 14, Pin name = IO_L20P_T3_A08)D24_14,				Sch name = CRAM_DQ2
#set_property PACKAGE_PIN U12 [get_ports {MemDB[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[2]}]
##Bank = 14, Pin name = IO_L5N_T0_D07_14,					Sch name = CRAM_DQ3
#set_property PACKAGE_PIN R13 [get_ports {MemDB[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[3]}]
##Bank = 14, Pin name = IO_L17N_T2_A13_D29_14,				Sch name = CRAM_DQ4
#set_property PACKAGE_PIN U18 [get_ports {MemDB[4]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[4]}]
##Bank = 14, Pin name = IO_L12N_T1_MRCC_14,					Sch name = CRAM_DQ5
#set_property PACKAGE_PIN R17 [get_ports {MemDB[5]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[5]}]
##Bank = 14, Pin name = IO_L7N_T1_D10_14,					Sch name = CRAM_DQ6
#set_property PACKAGE_PIN T18 [get_ports {MemDB[6]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[6]}]
##Bank = 14, Pin name = IO_L7P_T1_D09_14,					Sch name = CRAM_DQ7
#set_property PACKAGE_PIN R18 [get_ports {MemDB[7]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[7]}]
##Bank = 15, Pin name = IO_L22N_T3_A16_15,					Sch name = CRAM_DQ8
#set_property PACKAGE_PIN F18 [get_ports {MemDB[8]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[8]}]
##Bank = 15, Pin name = IO_L22P_T3_A17_15,					Sch name = CRAM_DQ9
#set_property PACKAGE_PIN G18 [get_ports {MemDB[9]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[9]}]
##Bank = 15, Pin name = IO_IO_L18N_T2_A23_15,				Sch name = CRAM_DQ10
#set_property PACKAGE_PIN G17 [get_ports {MemDB[10]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[10]}]
##Bank = 14, Pin name = IO_L4N_T0_D05_14,					Sch name = CRAM_DQ11
#set_property PACKAGE_PIN M18 [get_ports {MemDB[11]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[11]}]
##Bank = 14, Pin name = IO_L10N_T1_D15_14,					Sch name = CRAM_DQ12
#set_property PACKAGE_PIN M17 [get_ports {MemDB[12]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[12]}]
##Bank = 14, Pin name = IO_L9N_T1_DQS_D13_14,				Sch name = CRAM_DQ13
#set_property PACKAGE_PIN P18 [get_ports {MemDB[13]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[13]}]
##Bank = 14, Pin name = IO_L9P_T1_DQS_14,					Sch name = CRAM_DQ14
#set_property PACKAGE_PIN N17 [get_ports {MemDB[14]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[14]}]
##Bank = 14, Pin name = IO_L12P_T1_MRCC_14,					Sch name = CRAM_DQ15
#set_property PACKAGE_PIN P17 [get_ports {MemDB[15]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemDB[15]}]

##Bank = 15, Pin name = IO_L23N_T3_FWE_B_15,					Sch name = CRAM_A0
#set_property PACKAGE_PIN J18 [get_ports {MemAdr[0]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[0]}]
##Bank = 15, Pin name = IO_L18P_T2_A24_15,					Sch name = CRAM_A1
#set_property PACKAGE_PIN H17 [get_ports {MemAdr[1]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[1]}]
##Bank = 15, Pin name = IO_L19N_T3_A21_VREF_15,				Sch name = CRAM_A2
#set_property PACKAGE_PIN H15 [get_ports {MemAdr[2]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[2]}]
##Bank = 15, Pin name = IO_L23P_T3_FOE_B_15,					Sch name = CRAM_A3
#set_property PACKAGE_PIN J17 [get_ports {MemAdr[3]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[3]}]
##Bank = 15, Pin name = IO_L13P_T2_MRCC_15,					Sch name = CRAM_A4
#set_property PACKAGE_PIN H16 [get_ports {MemAdr[4]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[4]}]
##Bank = 15, Pin name = IO_L24P_T3_RS1_15,					Sch name = CRAM_A5
#set_property PACKAGE_PIN K15 [get_ports {MemAdr[5]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[5]}]
##Bank = 15, Pin name = IO_L17P_T2_A26_15,					Sch name = CRAM_A6
#set_property PACKAGE_PIN K13 [get_ports {MemAdr[6]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[6]}]
##Bank = 14, Pin name = IO_L11P_T1_SRCC_14,					Sch name = CRAM_A7
#set_property PACKAGE_PIN N15 [get_ports {MemAdr[7]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[7]}]
##Bank = 14, Pin name = IO_L16N_T2_SRCC-14,					Sch name = CRAM_A8
#set_property PACKAGE_PIN V16 [get_ports {MemAdr[8]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[8]}]
##Bank = 14, Pin name = IO_L22P_T3_A05_D21_14,				Sch name = CRAM_A9
#set_property PACKAGE_PIN U14 [get_ports {MemAdr[9]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[9]}]
##Bank = 14, Pin name = IO_L22N_T3_A04_D20_14,				Sch name = CRAM_A10
#set_property PACKAGE_PIN V14 [get_ports {MemAdr[10]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[10]}]
##Bank = 14, Pin name = IO_L20N_T3_A07_D23_14,				Sch name = CRAM_A11
#set_property PACKAGE_PIN V12 [get_ports {MemAdr[11]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[11]}]
##Bank = 14, Pin name = IO_L8N_T1_D12_14,					Sch name = CRAM_A12
#set_property PACKAGE_PIN P14 [get_ports {MemAdr[12]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[12]}]
##Bank = 14, Pin name = IO_L18P_T2_A12_D28_14,				Sch name = CRAM_A13
#set_property PACKAGE_PIN U16 [get_ports {MemAdr[13]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[13]}]
##Bank = 14, Pin name = IO_L13N_T2_MRCC_14,					Sch name = CRAM_A14
#set_property PACKAGE_PIN R15 [get_ports {MemAdr[14]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[14]}]
##Bank = 14, Pin name = IO_L8P_T1_D11_14,					Sch name = CRAM_A15
#set_property PACKAGE_PIN N14 [get_ports {MemAdr[15]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[15]}]
##Bank = 14, Pin name = IO_L11N_T1_SRCC_14,					Sch name = CRAM_A16
#set_property PACKAGE_PIN N16 [get_ports {MemAdr[16]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[16]}]
##Bank = 14, Pin name = IO_L6N_T0_D08_VREF_14,				Sch name = CRAM_A17
#set_property PACKAGE_PIN M13 [get_ports {MemAdr[17]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[17]}]
##Bank = 14, Pin name = IO_L18N_T2_A11_D27_14,				Sch name = CRAM_A18
#set_property PACKAGE_PIN V17 [get_ports {MemAdr[18]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[18]}]
##Bank = 14, Pin name = IO_L17P_T2_A14_D30_14,				Sch name = CRAM_A19
#set_property PACKAGE_PIN U17 [get_ports {MemAdr[19]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[19]}]
##Bank = 14, Pin name = IO_L24N_T3_A00_D16_14,				Sch name = CRAM_A20
#set_property PACKAGE_PIN T10 [get_ports {MemAdr[20]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[20]}]
##Bank = 14, Pin name = IO_L10P_T1_D14_14,					Sch name = CRAM_A21
#set_property PACKAGE_PIN M16 [get_ports {MemAdr[21]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[21]}]
##Bank = 14, Pin name = IO_L23N_T3_A02_D18_14,				Sch name = CRAM_A22
#set_property PACKAGE_PIN U13 [get_ports {MemAdr[22]}]
	#set_property IOSTANDARD LVCMOS33 [get_ports {MemAdr[22]}]
